Załącznik 1

**WYKAZ ASORTYMENTOWY**

**Serwer Dell PowerEdge 7615**

O specyfikacji:

* 2.5" Chassis with up to 16 SAS4/SATA Drives, Smart Flow, Front PERC 12
* Backplane SAS/SATA Capable
* Trusted Platform Module 2.0 V3
* AMD EPYC 9454 2.75GHz, 48C/96T, 256M Cache (290W) DDR5-4800
* 6 x 64GB RDIMM, 4800MT/s Dual Rank
* 4 x 1.6TB SSD SAS Mixed Use up to 24Gbps 512e 2.5in Hot-Plug 3DWPD , AG Drive
* Front H965i Rear Load
* BOSS-N1 controller card + with 2 M.2 480GB (RAID 1)
* iDRAC9, Enterprise szesnastej generacji
* No OCP 3.0 mezzanine NIC card, Blank Filler Only
* Broadcom 5720 Dual Port 1GbE Optional LOM
* Broadcom 57508 Dual Port 100GbE QSFP Adapter, PCIe Low Profile
* Riser Config 3, 2 x16 FH (Gen5) + 2 x8 FH + 2 x16 LP, Half Length
* PowerEdge 2U Standard Bezel
* ReadyRails™ Sliding Rails
* Dual, Hot-Plug, FR Power Supply, 1100W MM (100-240Vac) Titanium, Redundant (1+1)
* 2 x Rack Power Cord 2M (C13/C14 10A)
* No Operating System
* GPU/FPGA/ Acceleration Cards NVIDIA L4, PCIe, 72W, 24GB Passive, Single Wide Full Height GPU
* Basic Next Business Day 36 Months, 36 Mies.
* Keep Your Hard Drive For Enterprise, 36 Mies.

Elementy dodatkowe:

* 2 x Broadcom 57508 Dual Port 100GbE QSFP Adapter, PCIe Low Profile, Customer Kit
* 1 x Broadcom 57508 Dual Port 100GbE QSFP Adapter, PCIe Full Height, Customer Kit
* 1 x Riser with Two PCIe Gen3 FH slots, One x8 (slot 7) and 1 x16 (slot 8), min 2 processors, R740/XD CK
* 1 x Riser w/ 3 PCIe Gen3 slots, 1x16 FH (slot 4) ,1x8 FH (slot 5) and 1x8 LP (slot 6), min 2CPU, R740/XD CK
* 4 x Pamięć 32GB (3200MHz, DDR4 RDIMM, Dual Rank, ECC)
* 8 x Kabel QSFP28 DAC 3m SINGLE RATE 100GbE to 100GbE kodowany dla Broadcom 57508 z Cisco Catalyst C9500-48Y4C-A